## ReleaseVersion: [1.0.00000.233] - 2026-02-13

# Revision History

| Revision Number | Description | Revision Date |
| --------------- | ----------- | ------------- |
| 1.0.00000.233   | Release for Intel® PPM Provisioning Package driver WCL| WW08, 2026 |



<div style="page-break-before:always">&nbsp;</div>
<p></p>

# 1 Release Kit Summary

---

## 1.1 Release Kit Details

| Kit Release     | _Intel® PPM Provisioning Package Driver - 1.0.00000.233      |
| --------------- | ------------------------------------------------------------ |
| Target Platform | Wildcat Lake (WCL) Platofrm                                  |
| Contents        | Intel NULL Driver INF package with PPM ppkg and Release Notes|
| File Name       | PPMDRV-1.0.00000.233.zip                                      |

<div style="page-break-before:always">&nbsp;</div>
<p></p>

# 2 General Information

---

## 2.1 Important Notes

This Driver Contains PPM Package for 24H2 OS
| OS     | Package Name                    |
| ------ | --------------------------------| 
| 24H2   | PPM-Win11-24H2-WCL-v2026.0203113924.140dde8
| 23H2   |                          |
| Win10  | NA                           |                                     

## 2.2 Intended Audience

## 2.3 Supported OS

| OS Version | OS POR Platforms |
| ---------- | ---------------- |
| Windows 11 |   WCL	        |
| Windows 10 |   NA	        |




<div style="page-break-before:always">&nbsp;</div>


## 2.4 Acronyms


| Terms     |                                                                                           Description                                                                                           |
| :-------- | :---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------: |
| PPM 		|                                                              							Processor Power Management                                                                				  |
| IPF		|																						Intel® Platform Innovation Framework                                                                      |
| SoC       |                                                                                         System on Chip                                                                                          |
| WDK       |                                                                                       Windows Driver Kit                                                                                        |
| LNL       |                                                                                      Lunar Lake Platform                                                                                        |
| MTL       |                                                                                       Meteor Lake Platform                                                                                      |
| ADL       |                                                                                      Alder Lake Platform                                                                                        |
| PTL       |                                                                                      Panther Lake Platform                                                                                      |
| GNR       |                                                                                      Granite Rapids Platform                                                                                    | 
| WCL       |                                                                                      Wildcat Lake Platform                                                                                    |
| NVL       |                                                                                      Nova Lake Platform                                                                                    |
<div style="page-break-before:always">&nbsp;</div>

# 3 Introduction

---

#### This document specifies the driver release notes for Intel® PPM Provisioning Package driver, which exposed by IPF driver. This is NULL driver INF package and only purpose is to copy PPM ppkg into Windows Provisioning folder.


## 3.1 Document Scope

#### This document was written to guide on Intel® PPM Provisioning Package Driver releases for Windows OS (Nickel) on CCG platforms starting from WCL. This document will focus on the Driver package content, driver changes (feature implementations/fixes) and known limitations.


<div style="page-break-before:always">&nbsp;</div>


# 4 Intel® PPM Provisioning Package Driver Package

---

### <span style="color:#0860A8">**Driver Version: 1.0.00000.233**</span>


# 5 Supported Configuration

---

### <span style="color:#0860A8">**Target Platforms:**</span>

- #### WCL

### <span style="color:#0860A8">**Windows OS:**</span>

- #### 	SV2 Win11 22H2(x64) 
- ####  SV3 Win11 23H2(x64) 
- ####  SV4 Win11 24H2(x64) 
- ####  Win10 Supported


### <span style="color:#0860A8">**EWDK:**</span>

- #### NA


<div style="page-break-before:always">&nbsp;</div>


# 6 Known Limitations

---

- #### **PPM package may not get apply immediately after driver installation and might take around ~60min after system enter idle**
- #### **Also a reboot recommended after driver installation and please follow BKM described in next sections for how to expedite PPM provisioning after driver installation**

## BKM for expedite PPM provisioning after Driver installation

You can refer following BKM for applying PPM package immediately after reboot using Windows “Task Scheduler” (In case if you need to verify PPM settings).
- #### ** Open the Task Scheduler, select “Provisioning” and then select “RunOnReboot” and then click on “Enable” as show below image**

<img src="images/TTaskScheduler.png"></img>

<div style="page-break-before:always">&nbsp;</div>

-	#### ** Reboot the system**
-	#### ** Though above BKM guaranty PPM package will applied almost immediately after reboot, but if EPO (DTT Driver) load before Provisioning task start execute then still there could be a mismatch and hence it is recommended to do one more reboot before verify PPM settings**


#### **HSD’s:**

| ID        |                                                                        Title                                                                              |
| :-------- | :-------------------------------------------------------------------------------------------------------------------------------------------------------: |


<div style="page-break-before:always">&nbsp;</div>

# 7 HW Setup

---
No HW setup required/dependency and only pre-request is latest IPF driver with PPM support


# 8 BIOS Configuration

---
No BIOS dependency/Configuration required
